---
navigation:
  title: "エタノール"
  icon: "pneumaticcraft:ethanol_bucket"
  parent: pneumaticcraft:renewables.md
---

# エタノール

*エタノール*は[酵母培養液](./yeast_culture.md)と*砂糖*を使用して[熱空気圧処理プラント](../manufacturing/thermopneumatic_processing_plant.md)で生成できます。これは[バイオディーゼル](./biodiesel.md)の構成要素の1つです。

このプロセスは温度に敏感です。熱空気処理プラントの温度を30℃から60℃の間に保つ必要があります。

これは暖かいバイオームでは非常に簡単ですが、寒い地域では少し手間がかかるかもしれません。注意すべき点の1つは、深く掘るにつれて周囲の温度が上昇する傾向があるため、より低いYレベルで処理を実行する場合は温帯バイオームが適している可能性があることです。

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_sugar"}
```

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_melon"}
```

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_potato"}
```

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_poisonous_potato"}
```

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_apple"}
```

**TODO:** Unsupported Patchouli page type **pneumaticcraft:thermo_plant**

```
{"type":"pneumaticcraft:thermo_plant","recipe":"pneumaticcraft:thermo_plant/ethanol_from_sweet_berries"}
```

